

**Installation Guide:**

ALT-YD-TTU07V2-LB-(All)

Tools Needed:


* ¼” ratchet
* T30 Torx




1. Unseat tail light.



1. Remove (2x) T30 torx screws.



1. Remove bulb from brake socket.



1. Remove (3x) bulb sockets.



6. Seat (3x) bulb sockets onto Spyder tail light.



5.Install brake socket insert. (Align black wire from socket to black wire of socket insert)






1. Seat Spyder tail light.



1. Reinstall (2x) T30 Torx screws.





9.Turn on lights and confirm all functions are working properly. You have successfully completed the install of your new Spyder LED tail lights.



For further help with installation, please watch our installation video. Follow the direct link below to our YouTube channel for more information:

http://www.youtube.com/watch

**DISCLAIMER**

Spyder Auto Installation Guide is not liable for damages, injuries, and death while installing the product. This is intended to be an installation guide, to reduce installation time. We have no responsibility for improper installation. If you do not know how to install, please have a professional install it.