

**Installation Guide:**

ALT-YD-CS07-LED-(All)

Tools Needed:

* Phillips Screwdriver



1. Unseat tail light.




1. Remove (2x) phillips screws.



1. Remove bottom brake light bulb and replace with socket cap.



1. Remove (3x) bulb sockets from tail light. (Never touch bulbs with bare hands)



1. Install reverse socket into Spyder tail light.



1. Remove top brake lamp bulb. Install Spyder socket insert into brake socket. (Make sure socket plug black wire lines up with socket black wire)



1. Reinstall (2x) phillips screws securing tail light.



1. Seat Spyder tail light.



9. Turn on lights and confirm all functions are working properly. You have successfully completed the install of your new Spyder tail lights.



For further help with installation, please watch our installation video. Follow the direct link below to our YouTube channel for more information:

http://www.youtube.com/watch

**DISCLAIMER**

Spyder Auto Installation Guide is not liable for damages, injuries, and death while installing the product. This is intended to be an installation guide, to reduce installation time. We have no responsibility for improper installation. If you do not know how to install, please have a professional install it.